--------------------------------------------------------------------------------
CPU name:	Intel(R) Xeon(R) Gold 6248 CPU @ 2.50GHz
CPU type:	Intel Cascadelake SP processor
CPU clock:	2.49 GHz
--------------------------------------------------------------------------------
Initializing parameters...
Initializing atoms...
Creating atoms...
Pattern: seq
Number of timesteps: 200
Number of atoms: 256
Number of neighbors per atom: 1024
Number of times to replicate neighbor lists: 1
Estimated total data volume (kB): 1056.7680
Estimated atom data volume (kB): 3.0720
Estimated neighborlist data volume (kB): 1050.6240
Initializing neighbor lists...
Creating neighbor lists...
Computing forces...
Total time: 0.2466, Mega atom updates/s: 0.2076
Cycles per atom: 9631.9934, Cycles per neighbor: 9.4062
Statistics:
	Vector width: 16, Processor frequency: 2.0000 GHz
	Average neighbors per atom: 1018.9055
	Average SIMD iterations per atom: 63.6816
	Total number of computed pair interactions: 52428800
	Total number of SIMD iterations: 3276800
	Useful read data volume for force computation: 0.84GB
	Cycles/SIMD iteration: 150.4999
--------------------------------------------------------------------------------
Region force, Group 1: MEM_SP
+-------------------+------------+
|    Region Info    | HWThread 0 |
+-------------------+------------+
| RDTSC Runtime [s] |   0.085843 |
|     call count    |        200 |
+-------------------+------------+

+------------------------------------------+---------+------------+
|                   Event                  | Counter | HWThread 0 |
+------------------------------------------+---------+------------+
|             INSTR_RETIRED_ANY            |  FIXC0  |  129769100 |
|           CPU_CLK_UNHALTED_CORE          |  FIXC1  |  172300100 |
|           CPU_CLK_UNHALTED_REF           |  FIXC2  |  215371300 |
|              PWR_PKG_ENERGY              |   PWR0  |     9.2849 |
|              PWR_DRAM_ENERGY             |   PWR3  |          0 |
| FP_ARITH_INST_RETIRED_128B_PACKED_SINGLE |   PMC0  |          0 |
|    FP_ARITH_INST_RETIRED_SCALAR_SINGLE   |   PMC1  |     154000 |
| FP_ARITH_INST_RETIRED_256B_PACKED_SINGLE |   PMC2  |          0 |
| FP_ARITH_INST_RETIRED_512B_PACKED_SINGLE |   PMC3  |   89088000 |
|               CAS_COUNT_RD               | MBOX0C0 |       8354 |
|               CAS_COUNT_WR               | MBOX0C1 |       1126 |
|               CAS_COUNT_RD               | MBOX1C0 |       7863 |
|               CAS_COUNT_WR               | MBOX1C1 |       1105 |
|               CAS_COUNT_RD               | MBOX2C0 |       7990 |
|               CAS_COUNT_WR               | MBOX2C1 |       1113 |
|               CAS_COUNT_RD               | MBOX3C0 |       4775 |
|               CAS_COUNT_WR               | MBOX3C1 |       1112 |
|               CAS_COUNT_RD               | MBOX4C0 |       4201 |
|               CAS_COUNT_WR               | MBOX4C1 |       1127 |
|               CAS_COUNT_RD               | MBOX5C0 |       4035 |
|               CAS_COUNT_WR               | MBOX5C1 |       1120 |
+------------------------------------------+---------+------------+

+-----------------------------------+------------+
|               Metric              | HWThread 0 |
+-----------------------------------+------------+
|        Runtime (RDTSC) [s]        |     0.0858 |
|        Runtime unhalted [s]       |     0.0691 |
|            Clock [MHz]            |  1995.2787 |
|                CPI                |     1.3277 |
|             Energy [J]            |     9.2849 |
|             Power [W]             |   108.1610 |
|          Energy DRAM [J]          |          0 |
|           Power DRAM [W]          |          0 |
|            SP [MFLOP/s]           | 16606.5397 |
|          AVX SP [MFLOP/s]         | 16604.7458 |
|          Packed [MUOPS/s]         |  1037.7966 |
|          Scalar [MUOPS/s]         |     1.7940 |
|  Memory read bandwidth [MBytes/s] |    27.7476 |
|  Memory read data volume [GBytes] |     0.0024 |
| Memory write bandwidth [MBytes/s] |     4.9974 |
| Memory write data volume [GBytes] |     0.0004 |
|    Memory bandwidth [MBytes/s]    |    32.7450 |
|    Memory data volume [GBytes]    |     0.0028 |
|       Operational intensity       |   507.1471 |
+-----------------------------------+------------+

